MassHunter Workstation Acquisition for 6400 Series Triple Quad
LC/MS version B.05.00 Service Pack 1

Agilent Technologies
December 3rd 2012


-----------------------------------
Changes:
-----------------------------------
1) #198636 - 6490 LogAmp Timing Error on Acq B.05.00 with FW and B.04.01 SP4 with FW 6.36
2) #193935 - Instrument Configuration Report displays wrong instrument serial number 
3) #192258 - System is losing sensitivity after it is in standby mode for a while or when spray chamber is opened for cleaning
4) #189911 - Positive-Negative dMRM Performance is Improved with "Dummy" Transitions In B.05 (and B.04)
5) #198330 - Acquisition Time Stamps not always recorded at start of data acquisition
6) #199399 - Updating Retention Times (with MRM update tool) deletes Positive scan segments
7) #200779 - Fixed RFPAID's being corrupted by MH eMSEWrite atoms.

Including Changes from HotFix3
------------------------------
1) Firmware Fix for DMRM LC To Waste issue
	#193656 - During a run, divert the LC valve to waste does not function properly


2) Optimizer Fix for Presto Number - KEIO0803[2012-Aug03-013245]
	#195480 - Optimizer does not work for multiple-charged negative ion


3) Fix for “Excel Copy Issue for more than 200 transitions” or during “Apply, Run, Save and Save As”
	When a more than 200 transition table was copied from Excel to Acquisition, customers were seeing that 	some transitions were being lost and others were being duplicated when the method was saved. 
	This happens during Apply, Run, Save and Save As too . 
	TeamTrack #189114, #191180

4) Offline Method Editor Issues
	189904 - When “MassHunter Offline Method Editor Version B.05.00” is started while a data acquisition run is ongoing, acquisition 		is stopped! 
	192250 - Cannot see setting when open offline method editor

	192475 - Interactive sample run stops when close and re-open console
	 Worklist run stops when close and re-open of console 
	185315 - Acq Worklist shows Exception when User selects “View Acquisition Method” for completed sample (long Worklist))  

	192780 - Offline Method Editor creation uses online Driver 

	177032:  Entire UI of Offline Method Editor is in Read-only state when simulator are used 


5) #183594 - Fixed the problem of "Adjust" in the checktune report.


-----------------------------------
Files Changed:
-----------------------------------
1) Firmware 7.08


Below files will be installed into the C:\Program Files (x86)\Agilent\MassHunter\Workstation\Acq\bin folder
1) AgtQQQAcqMain.ocx		417 KB		8/17/2012 	3:04 PM
2) AgtQQQAcqDataSource.dll	893 KB		8/17/2012 	3:03 PM
3) AgtAcqMethodPane.dll		468 KB		8/21/2012 	6:53 PM
4) AgtOptOptimizer.dll		173 KB		9/24/2012 	11:26 AM
5) AgtQqQDeviceDriver.dll	484 KB		11/16/2012 	4:25 PM
6) AgtVoyEngCore.dll		168 KB		11/28/2012	8:44 PM
7) AgtQQQWorkflowUtility.dll	240 KB		12/3/2012	2:46 PM


Below files will be installed into the folders
C:\Program Files (x86)\Agilent\MassHunter\Workstation\Acq\ReportTemplates\QQQ\RDLTune and 
C:\Program Files (x86)\Agilent\MassHunter\Workstation\Acq\ReportTemplates\QQQ\RDLTune\6490
1) CheckTune.rdlc		46 KB		5/15/2012 9:16 AM
2) CheckTune_MS2.rdlc		46 KB		5/15/2012 9:16 AM
3) 6490\CheckTune.rdlc		46 KB		5/15/2012 9:16 AM
4) 6490\CheckTune_MS2.rdlc	46 KB		5/15/2012 9:16 AM



-----------------------------------
Instructions:
-----------------------------------
1) Copy executable (*.exe) to the local Hard Disk Drive (HDD) 

2) Right mouse click "Run as administrator".

3) Installation will install both the patch software and firmware.




	.
    .   o  .      Agilent Technologies
      . o .	  Life Sciences and Chemical Analysis 
  . o o   o o .   5301 Stevens Creek Blvd
      . o .	  Santa Clara, CA USA
    .   o   .	  95051 
	.




